BLACKMAGIC DESIGN ANNOUNCES NEW MICRO CONVERTER 12G MODELS

  New family of miniaturized and affordable broadcast converters   feature a new advanced design that supports all 12G-SDI formats up to 2160p60.

Fremont, CA, USA - Friday, November 12, 2021 - Blackmagic Design today announced a new family of Micro Converter 12G models that lets customers use HDMI equipment with professional SDI systems. These new models feature custom hardware developed by Blackmagic Design and include features previously only found on high end converters. Micro Converter 12G models include features such as 3D LUTs and more SD, HD and Ultra HD video formats.

Micro Converter 12G models are available immediately from Blackmagic Design resellers worldwide from US$109.

The new Blackmagic Micro Converters are incredibly tiny broadcast video converters that let customers connect between consumer HDMI and professional SDI equipment. The rugged and miniaturized design makes them small enough to be used anywhere. Customers get professional 3G-SDI or 12G-SDI connections, depending on the models, so customers can work with SD, HD and Ultra HD formats up to 2160p60. Micro Converters use USB for power, so they can be powered directly from televisions or laptop computers. Customers can even purchase them without power supplies. Only Blackmagic Micro Converters feature custom electronics that conform to global broadcast specifications, and can be updated to new standards in the future.

The Micro Converter SDI to HDMI 12G model is perfect for monitoring in all SD, HD, 4K and Ultra HD standards up to 2160p60. It includes a 17 point 3D LUT for color calibrating monitors. Customers can also output the 3D LUT on the 12G-SDI loop output. Plus it supports DCI film rates including 4Kp24, 4Kp47.95 and 4Kp48.

The Micro Converter SDI to HDMI 12G model is perfect for connecting HDMI cameras and computers to professional SDI equipment. Customers get two 12G-SDI outputs for connecting to SD, HD or Ultra HD equipment. When working in HD it supports 3G-SDI level A and B. This model also supports film standards including 4Kp24, 4Kp47.95 and 4Kp48.

The Micro Converter BiDirectional SDI/HDMI 12G model can convert in both directions, in different standards at the same time. Customers can convert SDI to HDMI and HDMI to SDI simultaneously. Plus it supports camera control protocol conversion, so customers can use Blackmagic Pocket Cinema Cameras with professional SDI live production switchers.

Unlike other small SDI converters, Blackmagic Micro Converters feature the highest quality broadcast technology, miniaturized into an incredibly strong metal enclosure. Each converter has the highest quality broadcast industry standard SDI and HDMI connectors. Blackmagic Micro Converters include a USB connection for power, as well as for changing settings via the converter utility on Mac and Windows. Because the USB powers the converter, customers can even power it from televisions or laptop computers. There are even LEDs for status. Customers can also buy Blackmagic Micro Converters with an AC power supply including 4 adapters for international use.

Unlike cheap converters, Blackmagic Micro Converters include the highest quality signal processing and deep bit depth video pipeline. Micro Converters have been engineered with precision electronics so customers get very low SDI jitter, allowing customers to extend SDI cables over long distances. That’s vital for live production where equipment such as cameras can be a long distance from switchers. Blackmagic Micro Converters work with both 8 and 10-bit video formats, in RGB or YUV, and in all SD, HD and Ultra HD formats, depending on the model, up to 2160p60. They even support 1080p24, 1080p47.95, 1080p48, 4Kp24, 4Kp47.95 and 4Kp48 film rates. Plus customers get fully embedded audio and timecode support.

For color accurate monitoring, some models include a 3D LUT. Customers can apply custom looks, color and gamma changes in real time for on set monitoring. Plus LUTs can also be applied to the SDI loop output, allowing customers to use the converter as a 3D LUT processor. 3D LUTs are great for allowing a low cost computer monitor or TV to be used as a color calibrated broadcast or grading monitor. 3D LUTs are included on the SDI to HDMI 3G, SDI to HDMI 12G and BiDirectional SDI/HDMI 12G models. Customers can even use DaVinci Resolve to create custom 3D LUTs. Because DaVinci Resolve can be downloaded free, it costs nothing to start creating their own library of 3D LUTs. Imagine reproducing old film stocks.

Micro Converter 12G models have everything for the latest HDR workflows. Simply connect a HDR monitor, projector or TV and customers are ready for HDR monitoring. Static metadata PQ and Hybrid Log Gamma (HLG) formats in the VPID are handled according to the ST2108-1, ST2084 and the ST425 standards. Micro Converter 12G models handle ST425 which defines 2 new bits in the VPID to indicate transfer characteristic of SDR, HLG or PQ. Plus the ST2108-1 standard defines how to transport HDR static or dynamic metadata over SDI. There is also support for ST2082-10 for 12G SDI as well as ST425 for 3G-SDI sources. Both Rec.2020 and Rec.709 colorspaces are supported.

Blackmagic Micro Converter 12G models add all the SDI and HD formats of the 3G models plus powerful Ultra HD and 4K formats. 12G-SDI formats include 2160p23.98, 2160p24, 2160p25, 2160p29.97, 2160p30, 2160p47.95, 2160p48, 2160p50, 2160p59.94, 2160p60, 4Kp23.98 DCI, 4Kp24 DCI, 4Kp25 DCI, 4Kp29.97 DCI, 4Kp30 DCI, 4Kp47.95 DCI, 4Kp48 DCI, 4Kp50 DCI, 4Kp59.94 DCI and 4Kp60 DCI, 4KPsF25 DCI, 4KPsF29.97 DCI and 4KPsF30 DCI. All these formats mean the Micro Converter 12G-SDI models have the film and television standards of the future so customers can move to Ultra HD whenever they want.

"Our Micro Converters are very popular and these new models are now using a custom design that runs Blackmagic OS so we can now include many more features than the old models could support because these new models are intelligent," said Grant Petty, Blackmagic Design CEO. "We think customers will love these new models and we look forward to releasing new software updates for them as we add even more new features!"

MICRO CONVERTER 12G FEATURES

  *  Extremely small design for portable operation.
  *  Supports upgrading software via USB connection.
  *  Includes 3D LUT for monitoring on SDI to HDMI model.
  *  Includes support for HDR via SDI and HDMI.
  *  Supports 12G-SDI and HDMI timecode standards.
  *  Features 12G-SDI technology with built in SDI re-clocking.
  *  Includes camera control features for Blackmagic ATEM switchers.
  *  Supports all video standards in NTSC, PAL, 720 HD, 1080 HD and 2160 Ultra HD.
  *  Models can be purchased with or without power supply.

AVAILABILITY AND PRICE

Micro Converter 12G models are available now from US$109, excluding local duties and taxes, from Blackmagic Design resellers worldwide.

PRESS PHOTOGRAPHY

Product photos of the Micro Converter 12G models, as well as all other Blackmagic Design products, are available at www.blackmagicdesign.com/uk/media/images.

ABOUT BLACKMAGIC DESIGN

Blackmagic Design creates the world’s highest quality video editing products, digital film cameras, color correctors, video converters, video monitoring, routers, live production switchers, disk recorders, waveform monitors and real time film scanners for the feature film, post production and television broadcast industries. Blackmagic Design’s DeckLink capture cards launched a revolution in quality and affordability in post production, while the company’s Emmy™ award winning DaVinci color correction products have dominated the television and film industry since 1984.

Blackmagic Design continues ground breaking innovations including 6G-SDI and 12G-SDI products and stereoscopic 3D and Ultra HD workflows. Founded by world leading post production editors and engineers, Blackmagic Design has offices in the USA, UK, Japan, Singapore and Australia. For more information, please go to www.blackmagicdesign.com/uk.

